DURAFLOR.COM

**M50 RUBBER/ PLASTICS/ CORK/ LINO/ CARPET TILING/ SHEETING  
110 VINYL SHEETING:**

**DURAGRIP SLIP-RESISTANT VINYL SHEETING**

In a range of exciting colours, Duragrip is a heavy contract slip-resistant vinyl sheeting that is ideal for heavy wear environments.

**Location:** Heavy use areas. Office, retail, hospitality, leisure and educational areas.

**Base:** Please refer to Duraflor installation guide for details of suitability.

**- Preparation:** Subfloors should be prepared in accordance with BS 5325 or corresponding National and European Standards.

**- Manufacturer:** Duraflor

Tel: 01592 630 030 | Email: [sales@duraflor.com](mailto:sales@duraflor.com) | Web: [www.duraflor.com](http://www.duraflor.com)

**- Product reference:** Duragrip

**- Type:** Vinyl, PVC

**BS EN 1307 classification:** 34

**Anti-slip Class DIN 51130:** R10

**Slip Resistance:**  RRL Pendulum Test (wet) - > 36

**Size:** Sheet 2m x 20m

**Colour/pattern:** As per finishes schedule

**Method of laying:** N/A

LONDON

47 Gee Street Clerkenwell London EC1V 3RS

LEEDS

Vitality House Milford Place Leeds LS4 2BQ

SCOTLAND

Unit 14 Faraday Road Glenrothes

KY6 2RU

01592 630 030

