DURAFLOR.COM

**M50 RUBBER/ PLASTICS/ CORK/ LINO/ CARPET TILING/ SHEETING
130 CARPET TILING:**

**NATURAL TERRAIN TUNDRA CARPET TILES**

Natural Terrain Tundra is a hard-wearing carpet tile and an excellent choice for heavy wear areas. It is available in a range of interwoven shades of greys and beiges.

**Location:** Heavy use areas. Office, retail, hospitality, leisure and educational areas.

**Base:** Please refer to Duraflor installation guide for details of suitability.

**- Preparation:** Subfloors should be prepared in accordance with BS 5325 or corresponding National and European Standards.

**- Manufacturer:** Duraflor

Tel: 01592 630 030 | Email: sales@duraflor.com | Web: [www.duraflor.com](http://www.duraflor.com)

**- Product reference:** Natural Terrain Tundra

 **- Type:** Solution Dyed Nylon

**BS EN 1307 classification:** 33

**Size:** 500mm x 500mm standard size.

**Colour/pattern:** As per finishes schedule

**Method of laying:** Brickbond

LONDON

47 Gee Street Clerkenwell London EC1V 3RS

LEEDS

Vitality House Milford Place Leeds LS4 2BQ

SCOTLAND

Unit 14 Faraday Road Glenrothes

KY6 2RU

01592 630 030

